DASSAULT FALCON 20E GE CF-700-2D
REFERENCE INFORMATION
For detailed instructions on how to fly this aircraft, see the Aircraft Information
articles in the Learning Center. For standard procedures, see the Checklists tab.

Total Flight Simulator aircraft weight with full fuel | 28,660 lbs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel and Load.

VMO - Maximum Operating Speed 23,400 Feet | 390 KNOTS
VMO - Maximum Operating Speed Sea Level | 350 KNOTS
MMO - Maximum Operating Speed Mach | 0.88 Mach
VA - Maneuvering Speed 27,320 lbs (sea level) | 200 KNOTS
Vmc – Min Control Speed 27,320 lbs (sea level) | 99 KNOTS (Flaps-10)
VLLO Landing Lights Extend speed | 190 KNOTS
VLO - Maximum Gear Operating Speed | 190 KNOTS
VLE - Maximum Landing Gear Extension Speed | 220 KNOTS
Limiting Tailwind componet | 10 KNOTS
Demonstrated crosswind componet | 25 KNOTS

Maximum Flap Placard Speeds

Flaps degrees | KNOTS
10 | 190
20 | 190
40 | 180

V1 - Takeoff Decision Speed dry runway
Standard temperature, sea level pressure altitude

All conditions | 107 KNOTS

VR - Rotation Speed dry runway
Standard temperature, sea level pressure altitude

23,000 lbs | 116 KNOTS
28,660 lbs | 120 KNOTS

Altitude Limitations
Standard temperature

Max TO/Landing | 10000 FEET
Max operating alt | 42000 FEET

VREF - Landing Approach Speed flaps 40, gear down
Standard temperature, sea level pressure altitude

23,000 lbs | 117 KNOTS
27,320 lbs | 120 KNOTS