[fltsim.0]
title=F86A_Sabre
sim=F86Sabre
model=
panel=
sound=
texture=
kb_checklists=
ui_manufacturer=North American
ui_type=F86Sabre
ui_variation=FU-257
atc_heavy=0
atc_id=
atc_airline=
atc_flight_number=
description=The North American F-86F Sabre was the most capable western fighter of the early- to mid-1950s. FU-257

[fltsim.1]
title=F86A_Sabre paint1
sim=F86Sabre
model=
panel=
sound=
texture=1
kb_checklists=
ui_manufacturer=North American
ui_type=F86Sabre
ui_variation=FU-764
atc_heavy=0
atc_id=
atc_airline=
atc_flight_number=
description=The North American F-86F Sabre was the most capable western fighter of the early- to mid-1950s. FU-764 

[General]
performance=Specification: Crew:1\nLength: 37ft 1in (11.4m)\nPowerplant: 1XGeneral Electric J47-GE-27 turbojet\nWingspan: 37ft (11.3m)\nHeight: 14ft 1in (4.5m)\nMax. speed: 687mph (1.106km/h)\nArmament: 6 guns 0.50 (12.7mm) Bombs 5,300lb (2.400Kg) 2X200 galons drop tanks and rockets
atc_type=
atc_model=
Category=airplane


[forcefeedback]
gear_bump_nose_magnitude=6000
gear_bump_nose_direction=18000
gear_bump_nose_duration=250000
gear_bump_left_magnitude=6000
gear_bump_left_direction=35500
gear_bump_left_duration=250000
gear_bump_right_magnitude=6000
gear_bump_right_direction=00500
gear_bump_right_duration=250000
ground_bumps_magnitude1=3250
ground_bumps_angle1=8900
ground_bumps_intercept1=5.0
ground_bumps_slope1=0.48
ground_bumps_magnitude2=750
ground_bumps_angle2=9100
ground_bumps_intercept2=0.075
ground_bumps_slope2=1.0
crash_magnitude1=10000
crash_direction1=01000
crash_magnitude2=10000
crash_direction2=9000
crash_period2=75000
crash_duration2=2500000


[ELECTRICAL]
max_battery_voltage=24.0
generator_alternator_voltage=28.0
max_generator_alternator_amps=50.0
;BusType, MaxAmpLoad, MinVoltage       BusTypes:0=MainBus,1=AvionicsBus,2=BatteryBus,3=HotBatteryBus,4-7=Generator/AlternatorBus(1-4)
flap_motor=0, 5 , 0.0
gear_motor=0, 5 , 0.0
autopilot=0, 5 , 0.0
avionics_bus=0, 10, 0.0
avionics=1, 5 , 0.0
pitot_heat=0, 2 , 0.0
additional_system=0, 20, 0.0
marker_beacon=1, 2 , 0.0
gear_warning=0, 2 , 0.0
fuel_pump=0, 5 , 0.0
starter1=0, 20, 0.0
light_nav=0, 5 , 0.0
light_beacon=0, 5 , 0.0
light_landing=0, 5 , 0.0
light_taxi=0, 5 , 0.0
light_strobe=0, 5 , 0.0
light_panel=0, 5 , 0.0

[LIGHTS]        
//Types: 1=beacon, 2=strobe, 3=navigation, 4=cockpit, 5=landing

light.1 = 3, -20.05,   0.08,  1.40, fx_navwhih ,
light.2 = 2,  -7.40, -18.60,  -0.40, fx_strobeh ,
light.3 = 2,  -7.40,  18.60,  -0.40, fx_strobeh ,
light.4 = 2, -20.05,  -0.08,  1.40, fx_beaconh ,
light.5 = 4,   7.65,   0.00,  2.50, fx_vclighth,
light.6 = 8, -16.70,   0.00, -0.00, fx_flame_T7,


[WEIGHT_AND_BALANCE]
//reference_datum_position=0.000000,0.000000,0.000000
//empty_weight_CG_position=0.000000,0.000000,0.000000
max_number_of_stations=50
station_load.0=0.000000,0.000000,0.000000,0.000000
empty_weight=8795.000
empty_weight_roll_MOI=100000.000
empty_weight_pitch_MOI=174039.000
empty_weight_yaw_MOI=251490.000
empty_weight_coupled_MOI=1300.000
reference_datum_position=0.000, 0.000, 0.000
empty_weight_CG_position=0.000, 0.000, 0.000
max_gross_weight=11810.000
CG_forward_limit=0.000
CG_aft_limit=1.000


[fuel]
LeftMain=0.000, 0.000, 0.000, 225.000, 0.000
RightMain=0.000, 0.000, 0.000, 225.000, 0.000
fuel_type=2.000000
number_of_tank_selectors=1
electric_pump=0


[airplane_geometry]
wing_area=342.000
wing_span=36.900
wing_root_chord=6.833
wing_dihedral=3.450
wing_incidence=-0.494
wing_twist=-1.000
oswald_efficiency_factor=121.353
wing_winglets_flag=0
wing_sweep=-8.170
wing_pos_apex_lon=0.000
wing_pos_apex_vert=0.000
htail_area=58.000
htail_span=16.500
htail_pos_lon=-23.167
htail_pos_vert=0.000
htail_incidence=0.000
htail_sweep=0.000
vtail_area=56.000
vtail_span=8.532
vtail_sweep=0.000
vtail_pos_lon=-23.167
vtail_pos_vert=5.750
elevator_area=25.250
aileron_area=14.440
rudder_area=9.350
elevator_up_limit=3.000
elevator_down_limit=3.000
aileron_up_limit=19.481
aileron_down_limit=14.897
rudder_limit=23.491
elevator_trim_limit=19.481
spoiler_limit=59.989
spoilerons_available=0
aileron_to_spoileron_gain=0.000
min_ailerons_for_spoilerons=0.000
min_flaps_for_spoilerons=0.000
auto_spoiler_available=1
spoiler_extension_time=0.800000
positive_g_limit_flaps_up=9.000000
positive_g_limit_flaps_down=9.000000
negative_g_limit_flaps_up=-9.000000
negative_g_limit_flaps_down=-9.000000


[contact_points]
point.0=1.000, 12.850,  0.000, -5.100, 1574.803, 0.000, 0.667,40.000, 0.250, 2.500, 0.850, 7.000, 6.000, 0.000, 0.000, 0.000
point.1=1.000, -1.800, -4.000, -5.100, 1574.803, 1.000, 0.667, 0.000, 0.305, 2.500, 0.785, 6.000, 8.000, 2.000, 0.000, 0.000
point.2=1.000, -1.800,  4.000, -5.100, 1574.803, 2.000, 0.667, 0.000, 0.305, 2.500, 0.785, 8.000, 6.000, 3.000, 0.000, 0.000
point.3=2.000, -8.250, -18.450, 0.000, 1574.803, 0.000, 0.000, 0.000, 0.000, 0.000, 0.000, 0.000, 0.000, 5.000, 0.000, 0.000
point.4=2.000, -8.250,  18.450, 0.000, 1574.803, 0.000, 0.000, 0.000, 0.000, 0.000, 0.000, 0.000, 0.000, 6.000, 0.000, 0.000
point.5=2.000,-18.000,  0.000, -1.310, 1574.803, 0.000, 0.000, 0.000, 0.000, 0.000, 0.000, 0.000, 0.000, 9.000, 0.000, 0.000
point.6=2.000, 15.100,  0.000,  1.000, 1574.803, 0.000, 0.000, 0.000, 0.000, 0.000, 0.000, 0.000, 0.000, 4.000, 0.000, 0.000

static_pitch=0.584
static_cg_height=4.850
gear_system_type=0



[Views]
eyepoint=9.163284,0.000000,1.999262


[GeneralEngineData]
engine_type=1
Engine.0=0.000, 0.000, 0.000
fuel_flow_scalar=1.000
min_throttle_limit=0.000000


[TurbineEngineData]
fuel_flow_gain=0.0025
inlet_area=9.250
rated_N2_rpm=15000.000
static_thrust=5200.000
afterburner_available=0
reverser_available=1


[Reference Speeds]
flaps_up_stall_speed=130.000
full_flaps_stall_speed=104.000
cruise_speed=482.302
max_indicated_speed=668.000000
max_mach=0.850000


[keyboard_response]
elevator=150.000000,250.000000
aileron=150.000000,250.000000
rudder=150.000000,250.000000


[autopilot]
autopilot_available=1
flight_director_available=0
default_vertical_speed=1800.000000
autothrottle_available=1
autothrottle_arming_required=0
autothrottle_takeoff_ga=0
autothrottle_max_rpm=90.000000
pitch_takeoff_ga=8.000000
use_no_default_bank=1
use_no_default_pitch=1
default_pitch_mode=0
default_bank_mode=0
max_pitch=10.000000
max_pitch_acceleration=1.000000
max_pitch_velocity_lo_alt=2.000000
max_pitch_velocity_hi_alt=1.500000
max_pitch_velocity_lo_alt_breakpoint=20000.000000
max_pitch_velocity_hi_alt_breakpoint=28000.000000
max_bank=25.000000
max_bank_acceleration=1.800000
max_bank_velocity=3.000000
max_throttle_rate=0.100000
nav_proportional_control=9.000000
nav_integrator_control=0.250000
nav_derivative_control=0.000000
nav_integrator_boundary=2.500000
nav_derivative_boundary=0.000000
gs_proportional_control=9.520000
gs_integrator_control=0.260000
gs_derivative_control=0.000000
gs_integrator_boundary=0.700000
gs_derivative_boundary=0.000000
yaw_damper_gain=0.000000


[direction_indicators]
direction_indicator.0=3,0


[jet_engine]
thrust_scalar=1.000


[flight_tuning]
cruise_lift_scalar=1.000
pitch_stability=1.000
roll_stability=1.000
yaw_stability=1.000
parasite_drag_scalar=1.000
induced_drag_scalar=1.000
elevator_effectiveness=1.000
aileron_effectiveness=1.000
rudder_effectiveness=1.000
elevator_trim_effectiveness=1.000
aileron_trim_effectiveness=1.000
rudder_trim_effectiveness=1.000


[Flaps.0]
type=1
span-outboard=0.500
extending-time=5.000
system_type=0
damaging-speed=0.000
blowout-speed=0.000
lift_scalar=1.000
drag_scalar=1.000
pitch_scalar=1.000
flaps-position.0=0.000, 0.000
flaps-position.1=13.331, 0.000
flaps-position.2=26.662, 0.000
flaps-position.3=39.992, 0.000


[brakes]
toe_brakes_scale=1.000031
parking_brake=1

[gear_warning_system]
gear_warning_available=1
pct_throttle_limit=0.099976
flap_limit_power=25.496622
flap_limit_idle=5.042029

[hydraulic_system]
electric_pumps=0
engine_map=1,0,0,0
normal_pressure=3000.000000

[stall_warning]
type=1
stick_shaker=1

[attitude_indicators]
attitude_indicator.0=1

[turn_indicators]
turn_indicator.0=1,0
[pitot_static]
pitot_heat=1.000000
[vacuum_system]
max_pressure=5.150000
vacuum_type=2
electric_backup_pressure=0.000000
engine_map=0,0,0,0
[pneumatic_system]
max_pressure=18.000000
bleed_air_scalar=1.000000
[deice_system]
structural_deice_type=0
