Real data and perfo rmance of Blackshape Bk100 Prime

WEIGHT |  |
MTOW | From 472.5 up to 620 kg |
Max baggage weight | 20 kg |
POWERPLANT |  |
Horsepower | 100 hp |
Engine | Rotax 912ULS3 |
Propeller | MTV-33-1A Var. Pitch |
DIMENSIONS |  |
Wingspan | 7.94 m |
Length | 7.18 m |
Height | 2.41 m |
Cabin Width | 0.76 m |
PERFORMANCES |  |
Takeoff run | From 150 up to 270 m |
Takeover 50 ft | From 300 up to 420 m |
Max Roc (MTOW, SL) | 1100 fpm |
Max operating altitude | 12000 ft |
Stall Speed With Flaps | From 35 up to 45 KCAS |
Max Level Speed (SL) | 152 KTAS |
Landing Groundroll | From 120 up to 150 m |
Load Factor | +4/-2 g |
Max endurance | 4.5 h |